OpenWrt

Derivate

LEDE

FreeWRT

Freifunk-Firmware

Gargoyle baut auf OpenWrt auf und ergänzt es um ein Webinterface mit vielen Funktionen

Tomato

Erweiterungen

X-Wrt Erweiterung für OpenWrt, liefert ein Webinterface für den Endbenutzer

Siehe auch

DD-WRT

Linksys WRT54GL

Tips & Tricks

Debrick

https://wiki.openwrt.org/doc/howto/generic.debrick

Beispiel: TP-Link Archer C50 v3

https://wiki.openwrt.org/toh/tp-link/archer-c50#debricking

https://wiki.openwrt.org/toh/tp-link/tl-wdr4300#de-brick_or_oem_installation_using_the_tftp_recovery

Hintergrund: The stock firware (3.13.33(130617)) features a TFTP recovery client in bootloader. To activate it press and hold WPS/Reset Button during powering on until WPS LED turns on. Connect computer to LAN1. Using TCPdump, you should see ARP requests from router having address 192.168.0.86 looking for address 192.168.0.66.

Set up your computer to address 192.168.0.66, netmask /24 (255.255.255.0). Code # ip addr add dev eth0 192.168.0.66/24 </Code>

Using TCPdump, you should now see request for new firmware image:

Vorgehen: Download Recovery: https://static.tp-link.com/Archer%20C50(EU)_V3_170608.zip

Wichtig! Nach dem Entpacken das bin-File preparieren („To prepare recovery file cut the first 0x200 (that is 512) Bytes from original firmware (This cut only header of firmware, Recovery need bootloader and firmware)“)

Grundsätzliche Vorgehensweise:

Setup your computer to 192.168.0.66 (SubnetMask /24 = 255.255.255.0) and connect it to LAN1.

Start TFTP server and provide recovery file with it.

To activate TFTP Recovery press and hold WPS/Reset Button during powering (8 sec.) on until WPS LED turns on.

Create directory where you want to put the image file

Put an image file into your directory

Change the ownership of the folder and the file in it

Run TFTP server

Check if your server is listening

Evtl. verhindert rlinetd das sraten, da er auf dem gleichen Port lauscht, dann hilft:

Check that you can in fact pull the file from your tftp server

Weblinks

de:OpenWrt

http://openwrt.org